# HG changeset patch
# User HackaLittleBit
# Date 1388680260 0
#      Thu Jan 02 16:31:00 2014 +0000
# Node ID b0402b37a4f748924f29ee309203c1832b03dfd8
# Parent  972ecec47c44188aa78f1ada76915b13679533a9
Set approach to touch-down distance to 8 tiles

diff --git a/src/table/airport_movement.h b/src/table/airport_movement.h
--- a/src/table/airport_movement.h
+++ b/src/table/airport_movement.h
@@ -56,8 +56,8 @@
 	AMD(   61,   40, AMED_EXACTPOS,                   DIR_NE), // 07 Taxi to start of runway (takeoff)
 	AMD(    3,   40, AMED_NOSPDCLAMP,                 DIR_N ), // 08 Accelerate to end of runway
 	AMD(  -79,   40, AMED_NOSPDCLAMP | AMED_TAKEOFF,  DIR_N ), // 09 Take off
-	AMD(  177,   40, AMED_HOLD       | AMED_SLOWTURN, DIR_N ), // 10 Fly to landing position in air
-	AMD(   56,   40, AMED_HOLD       | AMED_LAND,     DIR_N ), // 11 Going down for land
+	AMD(  176,   40, AMED_HOLD       | AMED_SLOWTURN, DIR_N ), // 10 Fly to landing position in air
+	AMD(   60,   40, AMED_HOLD       | AMED_LAND,     DIR_N ), // 11 Going down for land
 	AMD(    3,   40, AMED_NOSPDCLAMP | AMED_BRAKE,    DIR_N ), // 12 Just landed, brake until end of runway
 	AMD(    7,   40, 0,                               DIR_N ), // 13 Just landed, turn around and taxi 1 square
 	AMD(   53,   40, 0,                               DIR_N ), // 14 Taxi from runway to crossing
@@ -92,7 +92,7 @@
 	AMD(    7,   54, AMED_NOSPDCLAMP,                 DIR_N ), // 13 Release control of runway, for smoother movement
 	AMD(    5,   54, AMED_NOSPDCLAMP,                 DIR_N ), // 14 End of runway
 	AMD(  -79,   54, AMED_NOSPDCLAMP | AMED_TAKEOFF,  DIR_N ), // 15 Take off
-	AMD(  178,   54, AMED_HOLD       | AMED_SLOWTURN, DIR_N ), // 16 Fly to landing position in air
+	AMD(  189,   54, AMED_HOLD       | AMED_SLOWTURN, DIR_N ), // 16 Fly to landing position in air
 	AMD(   73,   54, AMED_HOLD       | AMED_LAND,     DIR_N ), // 17 Going down for land
 	AMD(    3,   54, AMED_NOSPDCLAMP | AMED_BRAKE,    DIR_N ), // 18 Just landed, brake until end of runway
 	AMD(   12,   54, AMED_SLOWTURN,                   DIR_NW), // 19 Just landed, turn around and taxi
@@ -135,7 +135,7 @@
 	AMD(   89,   85, AMED_EXACTPOS,                   DIR_NE), // 10 Taxi to start of runway (takeoff)
 	AMD(    3,   85, AMED_NOSPDCLAMP,                 DIR_N ), // 11 Accelerate to end of runway
 	AMD(  -79,   85, AMED_NOSPDCLAMP | AMED_TAKEOFF,  DIR_N ), // 12 Take off
-	AMD(  177,   87, AMED_HOLD       | AMED_SLOWTURN, DIR_N ), // 13 Fly to landing position in air
+	AMD(  205,   87, AMED_HOLD       | AMED_SLOWTURN, DIR_N ), // 13 Fly to landing position in air
 	AMD(   89,   87, AMED_HOLD       | AMED_LAND,     DIR_N ), // 14 Going down for land
 	AMD(   20,   87, AMED_NOSPDCLAMP | AMED_BRAKE,    DIR_N ), // 15 Just landed, brake until end of runway
 	AMD(   20,   87, 0,                               DIR_N ), // 16 Just landed, turn around and taxi 1 square // NOT USED
@@ -224,7 +224,7 @@
 	AMD(   60,    6, AMED_NOSPDCLAMP,                 DIR_N ), // 29 Release control of runway, for smoother movement
 	AMD(  105,    6, AMED_NOSPDCLAMP,                 DIR_N ), // 30 End of runway
 	AMD(  190,    6, AMED_NOSPDCLAMP | AMED_TAKEOFF,  DIR_N ), // 31 Take off
-	AMD(  193,  104, AMED_HOLD       | AMED_SLOWTURN, DIR_N ), // 32 Fly to landing position in air
+	AMD(  221,  104, AMED_HOLD       | AMED_SLOWTURN, DIR_N ), // 32 Fly to landing position in air
 	AMD(  105,  104, AMED_HOLD       | AMED_LAND,     DIR_N ), // 33 Going down for land
 	AMD(    3,  104, AMED_NOSPDCLAMP | AMED_BRAKE,    DIR_N ), // 34 Just landed, brake until end of runway
 	AMD(   12,  104, AMED_SLOWTURN,                   DIR_N ), // 35 Just landed, turn around and taxi 1 square
@@ -322,14 +322,14 @@
 	AMD(  134,   22, 0,                               DIR_SE), // 66 Taxi from runway 2in
 	AMD(  134,   38, 0,                               DIR_SE), // 67 Taxi from runway 2in
 	AMD(  134,   54, AMED_EXACTPOS,                   DIR_NE), // 68 Airport entrance2
-	AMD(  -58,    6, AMED_HOLD       | AMED_SLOWTURN, DIR_N ), // 69 Fly to landing position in air2
+	AMD(  -94,    6, AMED_HOLD       | AMED_SLOWTURN, DIR_N ), // 69 Fly to landing position in air2
 	AMD(   86,   38, 0,                               DIR_N ), // 70 Taxi Term group 2 exit - opp heli1
 	AMD(   70,   38, 0,                               DIR_N ), // 71 Taxi Term group 2 exit - opp heli2
 	AMD(   86,   55, AMED_EXACTPOS,                   DIR_SE), // 72 pre-helitakeoff helipad 1
 	AMD(   69,   54, AMED_EXACTPOS,                   DIR_NE), // 73 pre-helitakeoff helipad 2
 	AMD(    6,  118, AMED_HELI_RAISE,                 DIR_N ), // 74 Helitakeoff outside depot 1
 	AMD(  134,  102, AMED_HELI_RAISE,                 DIR_N ), // 75 Helitakeoff outside depot 2
-	AMD(  195,  166, AMED_HOLD       | AMED_SLOWTURN, DIR_N ), // 76 Fly to landing position in air1
+	AMD(  231,  166, AMED_HOLD       | AMED_SLOWTURN, DIR_N ), // 76 Fly to landing position in air1
 	AMD(  388,  -22, AMED_NOSPDCLAMP | AMED_SLOWTURN, DIR_N ), // 77 Initial DIAGDIR_NE approach
 	AMD(  310, -132, AMED_NOSPDCLAMP | AMED_SLOWTURN, DIR_N ), // 78 Initial DIAGDIR_SE approach
 	AMD( -352,   86, AMED_NOSPDCLAMP | AMED_SLOWTURN, DIR_N ), // 79 Initial DIAGDIR_SW approach
